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Apache Mall- Nimbus Playhouse
Option 2
Scope of Work

· Provide Architectural Drawings for permitting
· Demolition of walls noted on plan page A-200.03 of the “Nimbus Playhouse option 1”
· Demolition of walls and ACT ceiling in noted space on plan page A-200.03
· New Demising wall to deck- approx. 18’ tall wall as noted on plage page A-200.03
· New demising wall to be fire taped and sanded- No paint
· New sprinkler valve will be required to separate space
· Separate RTU for this space- Design by HVAC
· Extend 4” sanitary line from bathrooms into larger space
· Extend ¾” water line into this space.
· Bag all smoke detectors for demolition as noted on plan page A-200.03
· Temp lighting installed as noted on plan page A-200.03
· Separate electric for two spaces
· Separate sprinkler for two spaces
·  Option 2 to include the following:
· Demo approx. 20’ of demising wall to deck to create an opening to adjoining space as noted on plan pages A-000.03 and A-200.03
· Framing, drywall patching, and taping required where wall is opened up.
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