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Otto Wedding Venue- Building
Scope of Work
Demolition
· Demo of metal on exterior of existing 40 X 80 pole Building- Including Roofing
· Misc. Demolition of existing Electrical on walls
· Demo Two (2) Overhead Doors
Concrete
· New Concrete Footings and Foundation at 20 foot addition on the back of the building
· New Concrete Footings and Foundation at each 12’ x 100’ additions on each side of the existing building
· New Concrete Footings and Foundation at the 12 x 40 Vestibule Addition
· New Slab on grade concrete at all additions
· Concrete additions to get in floor heat
· New Concrete Stoops at Doors: 110B, 111A, 111D, 111C, 106A, 105A, 103, 101A, 100A, and 100B
· New Concrete at Trash Enclosure
· New Concrete at Mechanical Enclosure
· New Concrete Walk in front of Vestibule addition- Allowance for 5’ X 40’ 
· New Concrete Walk at Double Door 110B- Allowance for 12’ X 12’
· New Concrete Walk on West Side Addition- Allowance for 5’ X 100’
· New Concrete Walk on South Side Addition- Allowance for 5’ X 64’
Masonry- Stone
· New Stone Masonry on South Wall- See plan page A406

Steel
· New Steel Columns at Trash Enclosure and steel structure- Will attach Trex Decking or simar material.  Steel to be primed.- Figure Steel Columns with Base Plates
· New Steel Columns at Mechanical Enclosure and steel structure- Will attach Trex Decking or similar material.  Steel to be primed.- Figure Steel Columns with Base Plates
Lumber/Trusses/Metal Siding/Metal Roofing
· New Poles to continue pole Building at all additions.  Include base plates as all addition areas will receive footings and Foundations. **Please note on our website are pictures of the existing laminated posts. 
· Please note we haven’t been able to find any plans for the existing building
· New Trusses for 20’ addition on south end of building
· New Trusses for Vestibule addition
· New Trusses for 12’ X 100’ addition on East Side of Building
· New Trusses for 12’ X 100’ addition on West Side of Building
· New Metal Roof existing building and South Addition
· New Metal Roof on Vestibule Addition
· New Metal Roof on 12’ X 100’ East Side Addition
· New Metal Roof on 12’ X 100’ West Side Addition
· New Metal Siding on East Side Addition- Figure 4’ Wainscoting
· New Metal Siding on West Side Addition- Figure 4’ Wainscoting
· New Metal Siding on Vestibule Addition- Figure 4’ Wainscoting
· New Metal Siding on South Side addition- Figure 4’ Wainscoting
· New Acoustical Liner Paneling on Ceiling of Reception Hall
· Trex Decking for Trash and Mechanical Enclosures
· New Insulated Metal Exterior Doors: 106A, 105A, 103, 101A, 110B- Primed
· New Solid Core Wood Doors and Wood Casing for Doors: 106B, 105B, 104, 102, 101C, 101B- Staining by Others
· Pocket Doors: 109D, 109C- Staining by Others
· Barn Doors: 107, 108A, 108B, 109A, 109B, 110A- Staining by Others
· Two (2) Vinyl Window Type B- 4’ X 5’
· Seven (7) Vinyl Windows Type A- 3’ X 2’
· Tyvek wrap
· OSB for Sheer Wall- Current North Wall is a sheer wall, with the additions, figure new South Wall to be a Sheer Wall
Rough Carpentry labor
· Framing of all additions- Pole Building- New Poles will sit on new foundation walls
· Interior wall framing
· Installation of Windows
· Installation of Tyvek wrap on all exterior walls
· Installation of Metal Exterior Frames and Doors: 106A, 105A, 103, 101A
· Installation of Backing
· Installation of OSB for Sheer Wall
Finish Carpentry Materials
· Trim for Windows
· Trim for Wood Doors
Alternate: Shiplap on walls of Bar 108
Architectural Casework/Cabinetry
· Vanities for Bathrooms
· 18” Solid Surface (Corian or Similar) Countertop with Brackets in Brides Prep Area
· Solid Surface (Corian or Similar) Vanity Tops with integral bowls
· Granite Bar Top
· Cabinets with Solid Surface (Corian or Similar) in kitchen
· Wood Veneer paneling for front of bar
· PLAM Shelves with Brackes and Coat Bar in Vestibule
Insulation
· Poly ceiling of Reception Hall and insulate with Blown Insulation to Building code
· Spray Foam insulation on Exterior Walls- Base Bid
· Alternate: Batt insulation on Exterior Walls
· Chutes in attic
· Poly Ceiling in Vestibule and insulate with Blown Insulation to Building Code
· Rigid insulation installed at new Foundation Walls
Gutters and Down Spouts
· Supply and install gutters and down spouts on Roof of Reception Hall
· Supply and install gutters and down spouts on Roof of East Addition
· Supply and install gutters and down spouts on Roof of West Addition
· Supply and install gutters and down spouts on Roof of Vestibule Addition
Storefronts
· New Aluminum Storefront Doors: 100A, 100B, 111A, 111B, 111C, and 111D
· Two (2) New Aluminum Storefront Windows type C at vestibule- 8’ X 5’
Roll up Door/Shutter
· Roll up Door/Shutter at Pass through from Kitchen to Reception Hall- Manual operation
Drywall/Taping
· Supply, Hang, and Tape Drywall: Office 106, Grooms Prep 105, Men’s Restroom 104, Women’s Restroom 102, Hall 103, Brides Prep 101, Reception Hall 100, Mech & Storage 107, Bar 108, Kitchen 109, Delivery and Storage 110, and Vestibule 111.
· Supply, Hang, Tape/Texture ceilings: Office 106, Grooms Prep 105, Men’s Restroom 104, Hall 103, Women’s Restroom 102, Bride’s Prep 101, Mech. & Storage 107, Bar 108, Kitchen 109, Delivery and Storage 110, Vestibule 111.
Acoustical Ceilings
· Acoustical Ceiling in Kitchen 109
Painting/Staining
· Paint walls/Ceiling in: Office 106, Grooms Prep 105, Men’s Restroom 104, Hall 103, Women’s Restroom 102, Bride’s Prep 101, Bar 108, Vestibule 111.
· Paint Exterior Doors: 106A, 105A, 103, 101A, 110B
· Stain Interior Doors/Frames: 106B, 105B, 104, 102, 101C, 101B, 107, 108A, 108B. 109C, 109A, 109B, 110A
Alternate: Shiplap on walls of Bar 108
Tile
· Quarry Tile with Coved Base in Kitchen 109
· Ceramic Tile with coved base in Bar Area 108
· Ceramic Tile with coved base in Women’s Restroom 102
· Ceramic Tile with coved base in Men’s Restroom 104
Carpet Tile/Rubber Base
· Carpet tile with Rubber base in Bride’s Prep 101
· Carpet tile with Rubber baes in Grooms Prep 105
LVT/Rubber Base
· LVT with Rubber base in Office 106
· LVT with Rubber base in Vestibule 111
· Rubber Base in Delivery & Storage 110
Sealed Concrete
· Sealed Concrete in Mech. & Storage 107
Polished Concrete/Rubber Base
· Polished Concrete and Rubber Base in Reception Hall 100
· Polished Concrete and Rubber Base in Hall 103
Alternate Wood Base:
· Alternate for Wood Base:  Office 106, Groom’s Prep 105, Bride’s Prep 101, Reception Hall 100, Reception Hall 111
Toilet Partitions:
· Plastic Toilet and Urinal Partitions in Men’s Restroom 104
· Plastic Toilet Partitions in Women’s Restroom 102
Grab Bars/Bathroom Accessories
· Grab Bars and Bathroom Accessories in Bathrooms as noted on plans/Code Requirements
Fireplace
· Supply and install large Gas Fireplace on South Wall
· Include Mantel and trim- Prefinished Wood
FRP
· FRP on walls: Mech. & Storage 107, Delivery & Storage 110, and Kitchen 109
 Fire Protection Specialties: 
· Fire Extinguisher in Kitchen
· Two (2) Fire Extingusher with cabinets in Reception Hall 100
Food Service Equipment- to include design drawings
· Food Service Equipment to include but not limited to:
· Gas Range 
· Hand sinks
· Prep Sink 
· Work Tables
· Glass Washer
· Coolers
· Freezers
· Stainless Steel Pass through counter at pass through
· Ice Maker
· Microwave
Window Blinds
· Window Blind on Office Window
Plumbing/Gas Piping- Design Build
· Supply and install all toilets/Urinals
· Connection of plumbing to vanities
· Water Heater
· Boiler for In-Floor Heat
· In-Floor Heat- See plan page noting locations
· Grease Duct for kitchen hood- If Required by health department
· Floor Drains
· Kitchen Sink
· Plumbing to Bar Equipment
· Plumbing to Washing Machine
· Mop Sink
HVAC- Design Build
· Furnace/AC Units
· Ducting above ceilings
· Diffusers/return air grills in Acoustical Liner Paneling
· Diffusers/Return Air Grills in Acoustical Ceiling in kitchen
· Diffusers/Return Air Grills in drywall ceilings
Electrical- Design Build
· Provide new Electrical Service- Please note there are stub ups provided already- See pictures on our website
· Provide lighting in all areas of space
· Provide outlets for TV’s in reception hall and bar area
· Provide 3 large fans in reception area
· Provide electrical wall heater in Delivery & Storage 110
· Provide Exterior lighting- Sconces on Building
· Provide Exterior lighting on Building- Sconces  
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