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Apache Mall- Nimbus Playhouse
Option 1
Scope of Work

· Provide Architectural Drawings for permitting
· Demolition of walls noted on plan page A-200.03 of the “Nimbus Playhouse option 1”
· Demolition of walls and ACT ceiling in noted space on plan page A-200.03
· New Demising wall to deck- approx. 18’ tall wall as noted on plage page A-200.03
· New demising wall to be fire taped and sanded- No paint
· New sprinkler valve will be required to separate space
· Separate RTU for this space- Design by HVAC
· Extend 4” sanitary line from bathrooms into larger space
· Extend ¾” water line into this space.
· Bag all smoke detectors for demolition as noted on plan page A-200.03
· Temp lighting installed as noted on plan page A-200.03
· Separate electric for two spaces
· Separate sprinkler for two spaces
·  
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